Follows the procedure set forth in STSP 107-115 and requires submission of site specific safety plan prior to pre-con. Contact Environmental Coordinator before use.

1. Health and Safety Requirements for Workers Removing Contaminated River Sediment

*Add the following to standard spec 107.1:*

Contaminated sediment has been identified within the construction limits of this project. Based on sediment analytical data from investigations, contamination will be encountered during excavation and dewatering activities.

Site workers, that have a probability of exposure to a hazardous material, will have completed Health and Safety training that meets Occupational Safety and Health Administration (OSHA) requirements. Prepare a site-specific Health and Safety Plan complying with the OSHA standard for Hazardous Waste Operation and Emergency Response (HAZWOPER), 29 CFR 1910.120. Submit the site-specific Health and Safety Plan and written documentation of up-to-date OSHA training to the engineer before the pre-construction meeting.

Develop, delineate, and enforce the health and safety procedures pursuant to 29 CFR 1910.120, 29 CFR 1926.1101, and other heath and safety regulations. Restrict access to the Contaminated Material areas to only authorized, trained, and protected personnel until such time as excavation of contamination has been completed in the respective areas.

Specify the procedure for worker decontamination and for decontamination of equipment used in excavating, dewatering, and hauling of contaminated material in the site-specific Health and Safety Plan.

ner-107-085 (20180212)