Use when rumble strips are in asphaltic shoulders.

1. Removing Rumble Strips, Item SPV.0090.##

A Description

This special provision describes removing rumble strips by filling with Asphaltic Surface as the plans show. Conform to standard spec 465 and as follows.

B Materials

Asphaltic Surface conform to standard spec 465.

Tack Coat conform to standard spec 455.

C Construction

Before filling the existing rumble strip depressions, clean the depressions by sweeping, flushing, or using a stream of compressed air; then, coat the depressions with tack coat. Fill in the depressions with Asphaltic Surface. Overfill the rumble strips slightly and compact using a plate tamper or static roller so that the final compacted surface is flush with the existing pavement.

D Measurement

The department will measure Removing Rumble Strips by the linear foot.

E Payment

The department will pay for measured quantities at the contract price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0090.## Removing Rumble Strips LF

Payment is full compensation for all work under this item including cleaning the rumble strip depressions; furnishing and applying tack coat; and for furnishing and placing Asphaltic Surface.

ner-203-010 (20190710)