Use when rumble strips are in concrete shoulders.

1. Removing Rumble Strips, Item SPV.0180.##

A Description

This special provision describes removing existing rumble strips located in existing concrete shoulder as the plans show. Conform to standard spec 204, 465 and as follows.

B Materials

Asphaltic Surface Temporary conforming to standard spec 465.

Tack Coat conforming to standard spec 455.

C Construction

Mill the existing rumble strips to a 1-inch minimum depth conforming to standard spec 204. Clean the milled area to place tack coat conforming to standard spec 455.. Fill the milled area with Asphaltic Surface Temporary to provide for a smooth driving surface as the engineer directs.

Place Asphaltic Surface Temporary conforming to standard spec 465.

D Measurement

The department will measure Removing Rumble Strips in area by the square yard of existing rumble strips before removal by milling, acceptably completed.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0180.## Removing Rumble Strips SY

Payment is full compensation for milling existing rumble strips; cleaning; tacking; placing the compacting HMA concrete pavement; and for properly disposing of all materials.

ner-203-015 (20180221)