Discuss with PM before using.

1. Breaking Concrete Surface Drains, Item SPV.0180.##

A Description

This special provision describes breaking concrete surface drains to remain in place, at locations the plans show or as the engineer directs, and as follows.

B (Vacant)

C Construction

Crack the existing concrete slab completely through; it shall have a maximum dimension between fractures of three feet in any direction after cracking.

D Measurement

The department will measure Breaking Concrete Surface Drains by area in square yards of actual concrete cracked.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0180.## Breaking Concrete Surface Drains SY

Payment is full compensation for breaking concrete surface drains.

ner-204-005 (20171213)