1. Removing Cable Barrier, Item SPV.0090.##

A Description

This special provision describes removing the cable barrier as the plans show. Conform to standard spec 204 and as follows.

B (Vacant)

C Construction

Existing cable guard shall not be removed until temporary precast concrete barrier is in place between live traffic and the cable guard. All anchorages for cable barrier shall be removed.

D Measurement

The department will measure Removing Cable Barrier by the linear foot acceptably completed.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0090.## Removing Cable Barrier LF

Payment is full compensation for removing the cable barrier, posts and anchors.

ner-204-010 (20190710)