1. Removing Existing Underground Vault, Item SPV.0090.##

**A Description**

This special provision describes removing existing underground vault walls wholly and properly disposing of the resulting materials as the plans show. Conforming to standard spec 204 and as follows.

B Material

Supply a damp-proofing coating system on the exterior building foundation walls that will prevent moisture from passing through the foundations walls into the interior space.

Provide the manufacturer’s Certification of Compliance, product data sheet and installation instructions to the engineer at least 14 days before the work.

C Construction

Remove existing walls outside of building foundation wall entirely including any concrete floors. Existing building foundation walls shall be damp-proofed. Backfill all holes resulting from the removal of the existing vaults conforming to standard spec 209. Granular backfill will be paid for under the appropriate item as part of this contract.

**D Measurement**

The department will measure Removing Existing Underground Vault in length by the linear foot of vertical wall acceptably removed.

**D Payment**

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0090.## Removing Existing Underground Vault LF

Payment is full compensation for removing the vault; all saw cutting; for hauling and properly disposing of materials; and for damp-proofing the existing building foundation walls.

The department will pay for granular backfill under the appropriate bid item of the contract.

ner-204-020 (20190723)