Coordinate with Soils Engineer before using.

1. Embankment Construction - Benching.

*Replace standard spec 205.3.2(4) with the following:*

If placing embankment on side slopes 10-feet high or higher and steeper than one vertical to 3 horizontal, cut a minimum 18-inch depth bench into the existing embankment every 3 feet of vertical fill height.

ner-207-005 (20171213)