Coordinate with Soils Engineer before using.

1. Embankment Construction - Moisture Content

The moisture content of cohesive soils used in the construction of the roadway embankments shall not exceed optimum moisture content by more than 2% obtained from a standard proctor (AASHTO T99) for the material before proceeding with the placement of subsequent layers of the embankment construction.

On all embankments constructed of cohesive soils, perform compaction using specialized compaction equipment suitable for this type of soil, such as motorized sheepsfoot rollers.

ner-207-010 (20190717)