For use during construction before installation of permanent drains at bridge structures.

1. Temporary Slope Drain, Item SPV.0060.##

A Description

This special provision describes providing, maintaining, and removing a temporary slope drain to manage runoff from bridge decks before installation of surface drains, storm sewer, and pavement on the bridge approaches or permanent slope stabilization.

B (Vacant)

C Construction

Construct temporary slope drain conforming to the details shown in the plan and as required to fit the conditions of each location. Maintain the temporary slope drain at regular intervals or as the engineer directs. At a minimum maintain temporary slope drains until installation of permanent surface drains, storm sewer, and pavement are complete for bridges with finished approaches. Maintain the temporary slope drain at bridges without finished approaches or permanent drainage structures until downstream fill slopes are stabilized to prevent runoff scour.

D Measurement

The department will measure Temporary Slope Drain as each individual location installed conforming to the contract and accepted.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0060.## Temporary Slope Drain EACH

Payment is full compensation for furnishing and maintaining all materials; and for removal of the temporary slope drains.

ner-210-015 (20171213)