Coordinate with Pavement Engineer for use.

1. Concrete Joint and Crack Cleaning, Item SPV.0090.##

A Description

This special provision describes removing any loose or spalled concrete and asphaltic patching, cleaning the joints and cracks, and filling with asphaltic surface, as the plans show and as follows.

B Materials

Furnish asphaltic mixture as specified for asphaltic base under standard spec 315.2.

C (Vacant)

D Measurement

The department will measure Concrete Joint and Crack Cleaning by the linear foot along longitudinal and transverse joints and cracks, acceptably completed.

E Payment

The department will pay for the measured quantity at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0090.## Concrete Joint and Crack Cleaning LF

Payment is full compensation for removing and disposing of all loose or spalled concrete and asphaltic patching; for cleaning joints and cracks; for furnishing asphaltic material for filling the joints and cracks.

ner-415-030 (20171213)