Requires contractor to complete installation of endwalls within 7 calendar days of installing culvert pipe or box culvert.

1. Concrete Masonry Endwalls, Item 504.0900

*Add the following to standard spec 504.3:*

Concrete Masonry Endwalls shall be completed within 7 calendar days from the installation of each culvert pipe or box culvert location.

ner-504-005 (20180328)