Use this article with the NER construction detail for Culvert Pipe Concrete Collar only if SHES is necessary. If SHES not necessary, use item 520.8000 Concrete Collars for Pipe.

1. Culvert Pipe Concrete Collar SHES, Item SPV.0060.##

A Description

This special provision describes providing special high early strength concrete pipe collars. Conform to standard spec 520, as the plans show and as follows.

B Materials

Furnish and use SHES concrete masonry conforming to standard spec 416.2 as modified in standard spec 716. Provide QMP for class III ancillary concrete as specified in standard spec 716.

C Construction

Construct concrete collars per standard spec 520.3 and as the engineer directs.

D Measurement

The department will measure Culvert Pipe Concrete Collar SHES by the collar, acceptably completed.

E Payment

The department will pay for the measured quantity at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0060.## Culvert Pipe Concrete Collar SHES EACH

The department will pay for Culvert Pipe Concrete Collar SHES as specified in standard spec 520.5.

ner-520-005 (20190718)