Note to designer: This SPV is needed when shallow pipes need special backfill. See if Construction Detail Culvert Pipe with Transition and SPV Culvert Pipe Transition is needed with this SPV. Discuss with Soils Engineer for application.

1. Culvert Pipe Backfill, Item. 520.

For culvert pipes where depth from top of pipe to top of final pavement is 4.0-ft or less the entire backfill area will conform and be classified as standard spec 520.2.5.2 foundation backfill.

Remove standard spec 520.5.2(2) for culvert pipes described above. No extra pay items will be added for the substitution of foundation backfill for trench backfill.

Ner-520-010 (20190719)