000-Notes to designer: Use with the Construction Detail Culvert Pipe Transition. Removal of the triangle shape will be paid for as Common Excavation and if usable material should be shown in the earthwork table as such. There is an excel worksheet saved in the Design Resource Library in the Estimating folder for helping the designer calculate quantities for this operation. (DELETE FROM CONTRACT)

1. Foundation Backfill, Item SPV.0035.###.

A Description

This special provision describes providing foundation backfill that conforms to Standard Spec 520.

B Materials

Furnish Foundation Backfill in accordance to 520.2.5.2.

C Construction

Place foundation backfill in layers no more than 8 inches thick after compaction to the top of the subgrade. Mechanically compact the entire length of each layer to the same degree as the material abutting the trench.

D Measurement

The department will measure Foundation Backfill by the Cubic Yard, acceptably completed.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0035.### Foundation Backfill CY

Payment is full compensation for placing, shaping and compacting.

ner-520-025 (20190409)