Use when SHES concrete (8-hour cure time) is needed through driveway. Modify yellow sections if HES concrete (24-hour cure time) is needed.

1. Concrete Curb and Gutter 30-Inch SHES Type A, Item SPV.0090.##

A Description

This special provision describes providing concrete curb and gutter SHES with reinforcement. Conform to standard spec 601 for concrete curb and gutter.

B Materials

Furnish materials conforming to standard spec 601.2 except for concrete as specified in standard spec 416.2.

C Construction

All construction methods shall conform to standard spec 601.3.

D Measurement

The department will measure Concrete Curb and Gutter 30-Inch SHES Type A by the linear foot acceptably completed.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0090.## Concrete Curb and Gutter 30-Inch SHES Type A LF

The department will pay for Concrete Curb and Gutter 30-Inch SHES Type A as specified in standard spec 601.5.

ner-601-005 (20190718)