Use along OSOW routes where there will be vehicle over tracking of curb and gutter. Include construction detail in plan.

1. Concrete Curb and Gutter 4-Inch Sloped 30-Inch Type G Special, Item SPV.0090.##

A Description

This special provision describes providing cast-in-place concrete curb and gutter as the plans show. Conform to standard spec 601, and as follows.

B Materials

Furnish materials conforming to standard spec 601.2.

C Construction

All construction methods shall conform to standard spec 601.3.

D Measurement

The department will measure Concrete Curb and Gutter 4-inch Sloped 30-inch Type G Special by the linear foot acceptably completed as specified in standard spec 601.4.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0090.## Concrete Curb and Gutter 4-Inch Sloped 30-Inch Type G Special LF

The department will pay for Concrete Curb and Gutter 4-Inch Sloped 30-Inch Type G Special as specified in standard spec 601.5.

ner-601-010 (20190718)