1. Concrete Landscaping Curb, Item SPV.0090.##

A Description

This special provision describes providing special concrete curb of the dimensions and design the plans show, on the prepared foundation or base, at the locations and to the required lines and grades the plans show. Conform to standard spec 601 and as follows.

B Materials

All materials furnished and used in this item of work shall meet the requirements of standard spec 601 and as follows.

Batch all concrete from the same concrete plant with the same cement supplier throughout the project to prevent possible shade variance.

Tie bars shall conform to the requirements of standard spec 505.2.

C Construction

All work under this item shall conform to standard spec 601.3, and as follows.

Saw control joints as specified. Control joints shall match spacing of joints in adjacent concrete pad and curb and gutter.

D Measurement

The department will measure Concrete Landscaping Curb by the linear foot, in place and accepted.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0090.## Concrete Landscaping Curb LF

Payment is full compensation for all excavation and preparation of foundation, excluding the item of base aggregate dense; for furnishing all materials, including concrete masonry, expansion joints, and tie bars; for placing, finishing, protecting, and curing; for sawing of joints; for disposal of excess materials.

ner-601-020 (20190718)