Designer notes: Use this SPV when the design is dictating barrier is to be pinned. Do not use if the contractor has the option of constructing in a way that the barrier would not need to be pinned.

1. Concrete Barrier Temporary Precast Anchoring, Item SPV.0090.##.

A Description

This special provision describes anchoring temporary concrete barrier. Conform to standard spec 603 and as follows.

B Materials

Follow standard spec 603.

C Construction

Perform this work according to standard spec 603.3.2.1, the plans, and as hereinafter provided.

Under the Concrete Barrier Temporary Precast Anchoring bid item, furnish, deliver, and install anchors at the locations shown in the plans, as required by the project conditions, or as the engineer directs. Install anchors during the initial installation of the temporary concrete barrier and during any subsequent reinstallations of the temporary concrete barrier as required.

Remove any anchoring during barrier removal and fill remaining holes with epoxy.

D Measurement

The department will measure Concrete Barrier Temporary Precast Anchoring by the linear foot, acceptably completed, measured as the linear feet of barrier initially installed or reinstalled. The department will not measure anchoring made solely to accommodate the contractor's means and methods.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0090.## Concrete Barrier Temporary Precast Anchoring LF

Payment is full compensation for furnishing, delivering, and installing anchoring devices; for removal of any anchoring devices and filling holes with epoxy.

ner-603-010 (20180403)