Verify pipe material with community and verify testing requirements with materials section.

(DELETE FROM CONTRACT)

1. Mini Storm Sewer (Inch), Item SPV.0090.##; Mini Storm Sewer Lateral, (Inch), Item SPV.0090.##

A Description

This special provision describes providing mini storm sewer as the plan details show. Conform to standard spec 608 and as follows.

B Materials

Furnish the following pipe and lateral material: Polyvinyl chloride (PVC), ASTM Specification D-3034, SDR 35.

C Construction

All work under this item shall conform to standard spec 608.3.

D Measurement

The department will measure Mini Storm Sewer (Inch) and Mini Storm Sewer Lateral, (Inch), in length by the linear foot in place, and the quantity measured for payment shall be the horizontal distance measured along the centerline of the pipe from the inlet to the upstream end.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid items:

ITEM NUMBER DESCRIPTION UNIT

SPV.0090.## Mini Storm Sewer (Inch) LF

SPV.0090.## Mini Storm Sewer Lateral (Inch) LF

Payment is full compensation for furnishing all material including elbows, connections and cleanouts; for laying pipe; for connecting to inlets; for backfilling; and for furnishing granular backfill material.

ner-608-015 (20190718)