1. Storm Sewer Tap, Item SPV.0060.##

A Description

This special provision describes providing a storm sewer tap, as the plans show.

B Materials

Furnish grade A, A-FA, A-S, A-T, A-IS, A-IP or A-IT concrete conforming to standard spec 501 as modified in standard spec 716. Provide QMP for class III ancillary concrete as specified in standard spec 716.

Use granular backfill conforming to standard spec 209.

C Construction

Carefully saw hole to receive pipe in receiving pipe or structure.

Place pipe into receiving pipe or structure flush with interior wall.

Furnish and install the concrete encasement.

D Measurement

The department will measure Storm Sewer Tap as each individual unit acceptably completed.

E Payment

The department will pay for the measured quantity at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0060.## Storm Sewer Tap EACH

Payment is full compensation for furnishing, hauling and placing of all materials including the concrete encasement; and for excavating, backfilling, sawing, and disposing of excess material.

ner-608-040 (20190712)