Use this article for cover plates to remain in place.

1. Cover Plates, Item SPV.0060.##

A Description

This special provision describes providing steel plates to cover and support construction and traffic loadings at existing field inlets. Conform to standard spec 611, as the plans show, and as follows.

B Materials

Provide a 0.5-inch minimum thickness steel plate that extends to the outside edge of the existing masonry.

C Construction

Cover the portion of existing field inlets where proposed grading covers the existing grate. Cover plates will remain in place after completion of this project.

Clean out all soil, debris, other accumulated matter, and materials deposited or lodged due to the contractor’s operations from the structure before placing the cover plate on the structure. Place cover plate over portion of existing field inlet which is below the proposed ditch flow line elevation. Do not extend covers above the proposed flow line to prevent flow bypass of the inlet.

D Measurement

The department will measure Cover Plates as each unit, acceptably completed.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0060.## Cover Plates EACH

Payment is full compensation for cleaning out; and furnishing and installing the cover plate.

ner-611-015 (20171213)