Use in locations where only the adjustment rings need repair. Contact Maintenance before using.

1. Reconditioning Manholes, Item SPV.0060.##

A Description

This special provision describes reconditioning manholes. Conform to standard spec 519 and 611 and as follows.

B Materials

Conform to standard spec 519.2.

C Construction

Remove and replace all loose or deteriorated brick and mortar joints, mortar pipe connections that are not flush with the manhole, clean out the manhole, and apply a 1-inch mortar back plaster to the entire interior of the manhole at locations the plans show or as the engineer directs

D Measurement

The department will measure Reconditioning Manhole by each individual unit acceptably completed.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0060.## Reconditioning Manholes EACH

Payment is full compensation for furnishing required materials, including masonry; properly disposing of surplus material; and cleaning out and restoring the work site.

ner-611-060 (20190712)