This SDD slotted Vane Drain must accompany this SPV.

1. Repairing Slotted Vane Drain, Item SPV.0060.##

A Description

This special provision describes providing slotted vane drains, inlets, and surrounding concrete.

B Materials

Furnish materials conforming to standard spec 416 and standard spec 611.

C Construction

Remove damaged slotted vane drain grate and surrounding concrete as the engineer directs.

Salvage inlet cover and recondition inlet as the engineer directs.

Exercise care to avoid damage to the slotted vane drainpipe. If any section of pipe is damaged or is unsatisfactory as determined by the engineer, replace the drainpipe at contractor’s expense.

Before construction operations adjacent to the slotted area of the slotted vane drain pipe, cover the slots on the top of the drain. Remove any material entering the pipe at the contractor’s expense.

D Measurement

The department will measure Repairing Slotted Vane Drain as each individual unit acceptably completed.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0060.## Repairing Slotted Vane Drain EACH

Payment is full compensation for furnishing all materials; for removing and disposing of damaged slotted vane drain grate and surrounding concrete; for replacing slotted vane drain grate and concrete; and for salvaging inlet cover and reconditioning inlet.

ner-611-065 (20180424)