Used under temporary crossovers.

1. Temporary Pipe Underdrain Connections, Item SPV.0060.##

A Description

This special provision describes providing necessary temporary subsurface drainage at temporary traffic crossovers by placing designated temporary underdrain conforming to standard spec 612 and as follows.

B Materials

Furnish temporary unperforated corrugated steel pipe conforming to standard spec 612.2.2.

Furnish breaker to conform with standard spec 311.

Furnish Base Aggregate Dense to conform with standard spec 305.

C Construction

Salvage the existing rodent shield on the existing underdrain outfall. Connect the temporary unperforated corrugated steel pipe to the existing underdrain outfall and the temporary culvert pipe. Use corrugated steel tee connectors to connect the temporary unperforated corrugated steel pipe to the temporary culvert pipe. Backfill with breaker run or base aggregate dense.

Upon removal of the temporary traffic crossover, remove the temporary unperforated corrugated steel pipe and reinstall the rodent shield on the underdrain outfall.

D Measurement

The department will measure Temporary Pipe Underdrain Connections as EACH unit acceptably completed for the entire project.

E Payment

The department will pay for the measured quantity at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0060.## Temporary Pipe Underdrain Connections EACH

Payment is full compensation for providing, transporting, handling, and placing all materials including pipe, connections, and fittings; for salvaging and reinstalling rodent shields; and for removing the pipe upon removal of the temporary traffic crossover.

The department will pay separately for material required for backfill under the appropriate bid item.

ner-612-010 (20210716)