This article requires the use of steel posts instead of wood posts.

1. Steel Plate Beam Guard Class A

*Add to standard spec 614.2.1 the following:*

Steel Plate Beam Guard Class A installed along USH 41 shall be attached to steel posts and notched plastic blockouts.

ner-614-015 (20180516)