Coordinate with Landscape designer, can modify stone type and max/min aggregate size.

1. Mississippi River Gravel, Item SPV.0165.##

A Description

This special provision describes providing a weed barrier and Mississippi River Gravel as the plans show.

B Materials

Furnish nonwoven polypropylene geotextile fabric Type DF weed barrier conforming to spec 645.

Mississippi River Gravel shall be Wisconsin, Minnesota, or Iowa origin with a maximum stone size of 1 1/2 inches.

Visual inspect Mississippi River Gravel on site for size and soundness. Provide source of material.

C Construction

Place weed barrier in planting areas prior to placing Mississippi River Gravel. Overlap of weed barrier by a minimum of 3 inches.

Place Mississippi River Gravel to the final grades and a finished depth of 3 inches.

D Measurement

The department will measure Mississippi River Gravel, by the square foot acceptably completed.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid items:

ITEM NUMBER DESCRIPTION UNIT

SPV.0165.## Mississippi River Gravel SF

Payment is full compensation for preparing the foundation; furnishing, stockpiling, placing, compacting and shaping the Mississippi River Gravel.

The department will pay for Geotextile Type DF, separately.

ner-627-005 (20190710)