Item covers the cleaning and maintenance during use. Coordinate with Storm Water Engineer before using.

1. Temporary Stone Ditch Checks, Item SPV.0060.##

A Description

This special provision describes providing temporary stone ditch checks; cleaning and maintaining ditch checks as the plans show or as the engineer directs, and removing and disposing of the ditch checks as the engineer directs.

B Materials

Conform to standard specification 606.2.1 using the following gradation:

 VOLUME OCCUPIED

 INCHES BY STONES

 >8 0%

 4-6 50% - 90%

 <2 5% or less

Material shall be visually inspected and approved by the engineer.

C Construction

Place stone ditch checks immediately after shaping of the ditches or slopes are completed. Place stone checks at right angles to the direction of flow and construct conforming to the details shown in the plans.

Remove sediment from behind the stone ditch checks when it has accumulated to one half of the original height of the dam. Perform cleaning conforming to standard spec 628.

D Measurement

The department will measure Temporary Stone Ditch Checks by each item acceptably completed.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0060.## Temporary Stone Ditch Checks EACH

Payment is full compensation for furnishing, installing, maintaining, and cleaning; disposal of sediment; and for removing temporary ditch check.

Restoration of the area after ditch check removal shall be paid for with restoration items included in the contract.

ner-628-070 (20171213)