Use for perennials within roundabout or other landscaping areas. Coordinate use with Landscape designer.

1. Perennials, (Type), (Size), Item SPV.0060.##

A Description

This special provision describes providing perennial plantings at locations the plans show. Conform to standard spec 632 and as follows.

B Materials

Provide Perennial Plants, as shown on plan, and complying with American Standard for Nursery Stock (ANSI Z60.1-2004) for type, shape, and height.

Plant Materials. All plants shall be grown within the states of Wisconsin, Minnesota, Michigan, or parts of northern Illinois, Indiana or Ohio located within Zone 5 of the “Plant Hardiness Zone Map” produced by the United States Department of Agriculture, Miscellaneous Publication No. 1475, issued January, 1990, unless otherwise approved by the engineer.

Furnish a list of sources for plants as specified in standard spec 632.2.2.8 before planting begins for fall-planted plants and before March 15 for spring-planted plants. All sources will be subject to verification by the engineer.

Provide type B fertilizer.

C Construction

Ensure that Planting Mixture has been placed according to the standard specifications.

Stake out location of plantings for approval by supervising engineer.

Ensure that the bottom of the hole is adequately compacted to guard against settling. Tamp or water in as necessary to create a condition by which plants will not settle in the planting beds. The bottom of the rootball shall be in direct contact with the bottom of the hole.

Install Perennial Plants and mulching as the plans show.

D Measurement

The department will measure Perennials, (Type), (Size) by the unit acceptably complete in place.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid items:

ITEM NUMBER DESCRIPTION UNIT

SPV.0060.## Perennials, (Type), (Size) EACH

ner-632-010 (20171213)