Coordinate with Landscape designer.

1. Landscape Edging, Item SPV.0090.##

A Description

This special provision describes providing black polyethylene landscape edging at the locations the plans show.

B Materials

Landscape edging shall be black Polyethylene supplied in 20-foot minimum lengths.

Landscape edging shall be a minimum of 5 inches in depth with a double “V” anchor on the bottom edge and a hollow 1-inch diameter round top edge.

Landscape edging segments shall be joined at the top edge with manufacturer’s supplied fittings that fit securely into the hollow top edge of each length.

C Construction

Place Landscape edging in trench to a depth allowing the top edge to be 1” above finished grade.

Compact soil in trench so landscape edging is securely anchored in planting bed.

D Measurement

The department will measure Landscape Edging by the Linear Feet acceptably completed.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0090.## Landscape Edging LF

Payment is for providing and installing the edging and disposing of all excess and waste materials.

ner-645-015 (20190710)