Use this article when there will be an overlay. Be sure to revise HMA Pavement Type to match what will be used for the overlay.

1. Removing Raised Pavement Markers, Item SPV.0060.##

A Description

This special provision describes removing existing castings and filling original saw cut areas as the plans show or the engineer directs.

B Materials

Furnish materials conforming to standard spec 646.

C Construction

Remove existing pavement marker casting. Clean, dry and fill existing saw cut area with either epoxy or HMA Pavement (gradation) LT,MT or HT (Binder) (designation).

D Measurement

The department will measure Removing Raised Pavement Markers by the individual casting acceptably removed and filled with epoxy or HMA Pavement.

E Payment

The department will pay for the measured quantity at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0060.## Removing Raised Pavement Markers EACH

Payment for Removing Raised Pavement Markers is full compensation for removing, hauling, disposing of materials, and backfilling; cleaning and drying existing saw cut areas; and for furnishing and placing epoxy material or asphalt pavement.

ner-646-030 (20180619)