**4100-39-60 Work Description**

The proposed project will include the following work:

* 2-Inch mill of existing asphalt and pave 2-inches of HMA pavement
* Shape Shoulders and add shoulder gravel as needed
* Clean Culvert Pipes
* Retie end walls
* Add end walls
* Existing paved shoulders will be widened from 3 ft to 5 ft
* Centerline rumble strips
* Type 1 shoulder rumble strips
* New pavement markings will be installed
* Existing guardrail installations will be adjusted to meet current height requirements
* Paving to the face of beam guard
* Improper beamguard hardware replaced
* Damaged sections of rail will be replaced
* Grading behind EAT’s