|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Wetland No.** | **Fill Impact (ac)** | **Shading Impact (ac)** | **Total Impact (ac)** | **Comments** |
| 1 | 1.71 | 0.05 | 1.76 | CTH X bridge over Pebble Creek is approx. 8 ft. above ground surface. There is a 13.5 ft. gap between EB and WB structures. |
| 4 | 0.54 | 0.49 | 1.03 | Land bridge is approx. 3 ft. above ground surface. |
| 16  17 |  | 0.45\* | 0.57  0.86 | Bypass bridge over Pebble Creek is approx. 10 ft. above ground surface. There is a 15 ft. gap between NB and SB structures. |

\* The 0.45 ac. impact is for W-16 and W-17