{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":93,"n_cols":10,"rows_kept":93,"cut":false,"hidden":false,"merged":[]}
[1]
["Invert",1105.395,"Slope of pipe",{"$f":"(B2-B3)/B5","v":3.1937406855440081E-2}]
["Invert",1103.252,"Length of pipe at Centerline",34.299999999999997,null,"PIPE Thick","ELV at CL","CL ELV",null,"Cover Over Pipes in Feet"]
[null,null,"Flowline Elevation at CL",{"$f":"(D3*D2)+B3","v":1104.3474530551416},null,2,{"$f":"D4+F4","v":1106.3474530551416},1111.3800000000001,null,{"$f":"H4-G4","v":5.0325469448584954}]
["Length",67.099999999999994]
[]
[]
[]
[2]
["Invert",1239.146,"Slope of pipe",{"$f":"(B11-B10)/B13","v":3.8691216720578847E-2}]
["Invert",1240.701,"Length of pipe at Centerline",20.37,null,"PIPE Thick","ELV at CL","CL ELV",null,"Cover Over Pipes in Feet"]
[null,null,"Flowline Elevation at CL",{"$f":"(D11*D10)+B10","v":1239.9341400845981},null,2,{"$f":"D12+F12","v":1241.9341400845981},1244.51,null,{"$f":"H12-G12","v":2.5758599154019066}]
["Length",40.19]
[]
[]
[]
[3]
["Invert",1231.0319999999999]
["Invert",1227.5840000000001]
[]
["Length",50.49]
[]
[]
[]
[4]
["Invert",1212.3820000000001,"Slope of pipe",{"$f":"(B26-B27)/B29","v":9.3055801594334034E-2}]
["Invert",1207.1289999999999,"Length of pipe at Centerline",33.950000000000003,null,"PIPE Thick","ELV at CL","CL ELV",null,"Cover Over Pipes in Feet"]
[null,null,"Flowline Elevation at CL",{"$f":"(D27*D26)+B27","v":1210.2882444641275},null,2,{"$f":"D28+F28","v":1212.2882444641275},1218.02,null,{"$f":"H28-G28","v":5.7317555358724803}]
["Length",56.45]
[]
[]
[]
[5]
["Invert",1174.7719999999999,"Slope of pipe",{"$f":"(B34-B35)/B37","v":2.9542302357836801E-2}]
["Invert",1173.4939999999999,"Length of pipe at Centerline",19.760000000000002,null,"PIPE Thick","ELV at CL","CL ELV",null,"Cover Over Pipes in Feet"]
[null,null,"Flowline Elevation at CL",{"$f":"(D35*D34)+B35","v":1174.0777558945908},null,2,{"$f":"D36+F36","v":1176.0777558945908},1178.45,null,{"$f":"H36-G36","v":2.3722441054092087}]
["Length",43.26]
[]
[]
[]
[6]
["Invert",1031.1500000000001,"Slope of pipe",{"$f":"(B42-B43)/B45","v":6.4618456078083655E-2}]
["Invert",1028.2370000000001,"Length of pipe at Centerline",26.57,null,"PIPE Thick","ELV at CL","CL ELV",null,"Cover Over Pipes in Feet"]
[null,null,"Flowline Elevation at CL",{"$f":"(D43*D42)+B43","v":1029.9539123779948},null,2,{"$f":"D44+F44","v":1031.9539123779948},1038.1300000000001,null,{"$f":"H44-G44","v":6.1760876220052978}]
["Length",45.08]
[]
[]
[]
[7]
["Invert",984.21699999999998,"Slope of pipe",{"$f":"(B51-B50)/B53","v":4.279727606076518E-2}]
["Invert",986.66800000000001,"Length of pipe at Centerline",34.909999999999997,null,"PIPE Thick","ELV at CL","CL ELV",null,"Cover Over Pipes in Feet"]
[null,null,"Flowline Elevation at CL",{"$f":"(D51*D50)+B51","v":988.16205290728135},null,3,{"$f":"D52+F52","v":991.16205290728135},996.72,null,{"$f":"H52-G52","v":5.5579470927186776}]
["Length",57.27]
[]
[]
[]
[8]
["Invert",967.93,"Slope of pipe",{"$f":"(B59-B58)/B61","v":0.10700892857142903}]
["Invert",975.12099999999998,"Length of pipe at Centerline",35.61,null,"PIPE Thick","ELV at CL","CL ELV",null,"Cover Over Pipes in Feet"]
[null,null,"Flowline Elevation at CL",{"$f":"(D59*D58)+B59","v":978.93158794642852},null,3,{"$f":"D60+F60","v":981.93158794642852},985.4,null,{"$f":"H60-G60","v":3.4684120535714555}]
["Length",67.2]
[]
[]
[]
[9]
["Invert",920.46799999999996,"Slope of pipe",{"$f":"(B67-B66)/B69","v":0.16485595528164063}]
["Invert",931.97,"Length of pipe at Centerline",43.29,null,"PIPE Thick","ELV at CL","CL ELV",null,"Cover Over Pipes in Feet"]
[null,null,"Flowline Elevation at CL",{"$f":"(D67*D66)+B66","v":927.60461430414216},null,2,{"$f":"D68+F68","v":929.60461430414216},936.88,null,{"$f":"H68-G68","v":7.2753856958578353}]
["Length",69.77]
[]
[]
[]
[10]
["Invert",737.67,"Slope of pipe",{"$f":"(B74-B75)/B77","v":4.6272493573259891E-3}]
["Invert",737.47199999999998,"Length of pipe at Centerline",24.78,null,"PIPE Thick","ELV at CL","CL ELV",null,"Cover Over Pipes in Feet"]
[null,null,"Flowline Elevation at CL",{"$f":"(D75*D74)+B75","v":737.58666323907448},null,4,{"$f":"D76+F76","v":741.58666323907448},744.29,null,{"$f":"H76-G76","v":2.703336760925481}]
["Length",42.79]
[]
[]
[]
[11]
["Invert",701.45100000000002,"Slope of pipe",{"$f":"(B83-B82)/B85","v":2.1987577639751798E-2}]
["Invert",702.51300000000003,"Length of pipe at Centerline",26.94,null,"PIPE Thick","ELV at CL","CL ELV",null,"Cover Over Pipes in Feet"]
[null,null,"Flowline Elevation at CL",{"$f":"(D83*D82)+B82","v":702.0433453416149},null,2,{"$f":"D84+F84","v":704.0433453416149},705.59,null,{"$f":"H84-G84","v":1.5466546583851368}]
["Length",48.3]
[]
[]
[]
[12]
["Invert",694.73299999999995,"Slope of pipe",{"$f":"(B90-B91)/B93","v":3.7278314310797776E-2}]
["Invert",692.61,"Length of pipe at Centerline",34.71,null,"PIPE Thick","ELV at CL","CL ELV",null,"Cover Over Pipes in Feet"]
[null,null,"Flowline Elevation at CL",{"$f":"(D91*D90)+B91","v":693.90393028972778},null,2.5,{"$f":"D92+F92","v":696.40393028972778},700.81,null,{"$f":"H92-G92","v":4.4060697102721633}]
["Length",56.95]