000-Notes to designer: Use this spv for all contracts not on a freeway or expressway. The following language will aid in providing some definition of work zone clear zone restrictions for the contractor.

This article may not be applicable for some urban projects.

Insert this in the Traffic article.

Coordinate with work zone engineer for appropriate clear zone. Make sure your project can accommodate with in the right of way and other project specific restrictions.

(DELETE FROM CONTRACT)

1. Temporary Work Zone Clear Zone Working Restrictions.

Park equipment and store materials, including stockpiles, a minimum of XX-feet from the edge of the traveled way unless protected by concrete barrier temporary precast.

If the contractor is unsure whether an individual work operation will meet the safety requirements for working within the clear zone, review the proposed work operation with the engineer before proceeding with the work.

ner-104-005 (20200227)