000-Notes to designer: Note to be added to the Prosecution and Progress if need on project (DELETE FROM CONTRACT)

At the end of each work day, there cannot be a drop-off 2 inches or greater between the driving lanes and abutting surfaces that are for vehicle use.