On the plan identify what Seeding and fertilizer is anticipated. Add an Information only table showing the anticipated quantities for the Common, Borrow, Topsoil, E-mat, Fertilizer and Seeding.

1. Grading and Shaping Ditch, Item SPV.0090.##

A Description

This special provision describes excavating, filling, grading, shaping, compacting and finishing as necessary to improve slopes and provide positive drainage as the plans show and as follows.

B Materials

Furnish materials conforming to the following:

Common excavation and material disposal 205.2

Borrow 208.2

Topsoil 625.2

Erosion mat 628.2

Fertilizer 629.2

Seeding 630.2

C Construction

Grade, shape and finish the flowline of the ditch to provide positive drainage at the locations the plan show. Construct as plans show and engineer directs conforming to the following:

Common excavation and material disposal 205.3

Borrow 208.3

Topsoil 625.3

Erosion mat 628.3

Fertilizer 629.3

Seeding 630.3

D Measurement

The department will measure Grading and Shaping Ditch by the linear foot acceptably completed.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0090.## Grading and Shaping Ditch LF

Payment is full compensation for providing positive draining ditches at locations called out in the plan including required excavation, borrow, topsoil, e-mat, fertilizer and seeding when the ditch is outside of the contract grading limits. If the work specified above falls within the contract grading limits, the department will pay separately for that work under the excavation, borrow, topsoil, erosion mat, fertilizer and seeding bid items.

ner-205-005 (20180222)