Insert into all contracts with roadway foundation preparation

1. Preparing the Foundation

*Add the following to standard spec 211.3.1:*

The contractor shall plan construction activities such that the earth subgrade is covered by the roadway base in a timely manner upon completion of preparation of the subgrade or as the engineer directs. The contractor is responsible for the removal of any excess water from the subgrade as a result of rainfall events or natural drainage.

ner-211-005 (20171213)