For late season paving where the Contractor was forced. This item pays for the items that would normally be incidental for appropriate pricing. Include the type of covering in the item name (Plastic 1 layer, plastic 2 layers, plastic/hay/plastic or blanket, etc).

1. Concrete Pavement, Cold Weather Covering, (Type), Item SPV.0180.##

A Description

This special provision describes providing concrete paving protective covering conforming to standard spec 415.3.13, the plans, and as follows.

B Materials

Furnish materials that meet the requirements specified in standard spec 415.3.13.2.

C Construction

All work under this item shall conform to standard spec 415.3.13.

D Measurement

The department will measure the Concrete Pavement Cold Weather Covering (Type) in area by the square yard acceptably completed.

E Payment

The department will pay for the measured quantities at the contract unit price under the following bid items:

ITEM NUMBER DESCRIPTION UNIT

SPV.0180.## Concrete Pavement, Cold Weather Covering, (Type) SY

Payment is full compensation for supplying the plastic, hay, and material sufficient to weight down the insulating materials to withstand wind; and for furnishing all labor, tools, equipment, and incidentals required to place, remove, replace, and dispose of all covering materials as required during normal concreting operations. Heating of water or aggregates, or both, if deemed necessary by the contractor to maintain placement temperature, is incidental to this item.

ner-415-005 (20190717)