Verify pipe material with community and verify testing requirements with materials section.

(DELETE FROM CONTRACT)

1. Mini Storm Sewer Cleanouts, Item SPV.0060.##

A Description

This special provision describes providing mini storm sewer cleanouts as the plans show. Conform to standard spec 612 and as follows.

B Materials

Furnish pipe and fittings that meet the requirements for Type PSM Polyvinyl Chloride (PVC) Sewer Pipe (SDR 35) as set forth in ASTM Designation D-3034.

C Construction

Install mini storm sewer cleanouts in conforming to standard spec 612.3.

D Measurement

The department will measure Mini Storm Sewer Cleanouts by the unit, acceptably completed in place.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0060.## Mini Storm Sewer Cleanouts EACH

Payment is full compensation for furnishing and installing, transporting, handling and placing all materials, including pipe, backfill, connections, fittings, frost sleeve and caps or plugs; and for performing all excavation, compaction, proper disposal of surplus material and restoring the site of work.

ner-608-020 (20190718)