Use this for storm sewer plugs required for temporary extensions, staged construction, etc.

1. Storm Sewer Plug, Item SPV.0060.##

A Description

This special provision describes installing storm sewer plugs at locations the plans show.

B Materials

Provide a precast reinforced concrete plug or an engineer approved alternative, conforming to the inside diameter of the corresponding pipe as shown on the plan.

All materials, if concrete, must conform to standard spec 501 and standard spec 611.

C Construction

Place a watertight plug in the end of the storm sewer pipe in a manner that seals the pipe but allows for future removal of plug without damaging the storm sewer pipe.

D Measurement

The department will measure Storm Sewer Plug as each individual unit acceptably completed.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0060.## Storm Sewer Plug EACH

Payment is full compensation for providing storm sewer plugs and for removing when no longer needed.

ner-608-035 (20190718)