Item requires the use of only precast sections.

1. Manholes (dimensions).

Conform to standard spec 611 except furnish only precast structures.

ner-611-035 (20180423)