Requires stockpiling of endwalls to be picked up by Municipality

1. Salvaged Pipe Underdrain Endwalls, Item SPV.0060.##

A Description

This special provision describes removing, storing and replacing the existing endwalls.

B Materials

When lengthening the existing pipe underdrain is necessary, use unperforated pipe underdrain with a diameter that matches the existing pipe. Use material conforming to standard spec 612.

C Construction

Remove and store the salvaged endwalls at a safe location until the endwalls are ready to be mounted again in the newly constructed or extended drainage pipe.

When salvaging endwalls attached to pipe underdrain, if necessary, shorten or extend the pipe underdrain so that the uppermost section of the endwall is flush with the median slope.

Remove, store and install the salvaged endwalls in a manner as to preclude damage to the endwalls. Replace any items designated for salvage that are damaged by the contractor at no expense to the department.

Stockpile endwalls that are removed between Stations 245+00 and 285+00, but not reused elsewhere on the project, at a safe location for removal by the Winnebago County Highway Department. Contact the county when the endwalls can be removed. Dispose of any endwalls that are not salvaged by the county.

D Measurement

The department will measure Salvaged Endwalls, completed conforming to the contract and accepted, by the unit.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0060.## Salvaged Endwalls EACH

Payment is full compensation for removing, transporting, storing and installing the existing endwalls; and for shortening or lengthening the existing underdrain as necessary.

ner-612-005 (20171213)