Designer needs to verify with roadway maintenance engineer what cable guard system the county uses and the county contact. Part description and quantities need to match the system being used.

(DELETE FROM CONTRACT)

1. Parts for HT 4-Strand Cable Guard TL-4, Item SPV.0060.##

A Description

This special provision describes furnishing and delivering spare parts and tools for high-tension 4-strand cable guard barrier and terminals. The department and Brown County, hereinafter referred to as county, will use the parts and tools for maintaining and repairing the cable guard barrier and terminals after completion of construction.

B Materials

B.1 General

Furnish and deliver parts for 4-strand HT Cable Guard TL-3 Terminal and for NUCOR 4-cable Wire Rope Barrier System, both as specified by the manufacturer:

Nucor Steel Marion, Inc.

Highway Safety Products

912 Cheney Avenue, Marion, Ohio, 433-1801

Phone: (800) 333-4011

Contact: Chris Sanders, District Sales Manager

912 Cheney Ave., Marion, OH 43302

phone: (740) 383-9637, fax: (740) 383-6429

E-mail: [chris.sanders@nucor.com](mailto:chris.sanders@nucor.com).

The engineer will reject all non-conforming material.

B.2 List of Parts

Furnish the parts for Terminal 4-Strand HT Cable Guard TL-3, and Barrier 4-Strand HT Cable Guard Socketed TL-4 shown in the following list:

Description Quantity Unit

Line Posts 30 EACH

Small Hook Bolts w/Nuts 30 EACH

Large Hook Bolts w/Nuts 30 EACH

Hangers 30 EACH

Straps 30 EACH

CRP Top Post 4 EACH

CRP Bottom Post 4 EACH

1-Inch Turnbuckles 2 EACH

1-Inch Cable End Anchors 4 EACH

3/4-Inch Pre-Stretched Cable 2000 Ft. (1-Spool)

C Construction

C.1 Delivery of Parts and Tools

Deliver the parts listed in section B.2 of this special provision to the following location:

Brown County Maintenance Shop

2198 Glendale Avenue, Green Bay, WI, 54303.

County Contact person is:

Ed Kazik, Patrol Superintendent

cell phone: (920) 680-0409, work phone (920) 662-2166

Deliver the parts in a manner that is acceptable to the county and to the engineer. Contact the county ten working days before delivery to arrange for county personnel to be present during delivery.

D Measurement

The department will measure Parts for HT 4-strand Cable Guard TL-4 as EACH unit for the entire project, acceptably completing Parts for HT 4-strand Cable Guard TL-4.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0060.## Parts for HT 4-strand Cable Guard TL-4 EACH

Payment is full compensation for furnishing and delivering all materials listed in section B.2 of this special provision.

ner-614-010 (20210716)