“No-Mow” seed comes in two different mixes, one with rye and one without. Rye is added to provide rapid soil stability for seeding steep slopes and erosion prone sites. If you need rye another mix is needed otherwise a PIF is needed for a proprietary product. Eco-Grass does not have a mix that includes rye seed. Discuss with Regional REC person for need of rye on the project.

1. Low Maintenance Seed Mix, Item SPV.0085.##

A Description

This special provision describes furnishing and sowing low-maintenance seed at the locations the plans show. Conform to standard spec 630 and as follows.

B Materials

Furnish one of the following seed mixes: “No-Mow” seed mix as produced by Prairie Nursery, Westfield, Wisconsin; “Eco-Grass” as produced by Prairie Moon Nursery, Winona, MN; or an approved equal.

C Construction

Prepare the seed bed conforming to standard spec 630.3.2. Sow the seed mix conforming to standard spec 630.3.3. Sow seed at a rate that is conforming to the manufacturer’s recommendations.

D Measurement

The department will measure Low Maintenance Seed Mix by the pound in place.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0085.## Low Maintenance Seed Mix LB

Payment is full compensation for performing the work as described in 630.5 of the standard specification.

ner-630-005 (20190709)