1. Construction Staking Water Main, Item SPV.0060.##

A Description

This special provision describes the survey required to layout and construct all water main work included in this contract, including but not limited to water main, valves, water manholes, fittings, and hydrants.

B (Vacant)

C Construction

Perform the work conforming to 3.2.1 of the Standard Specifications for Sewer and Water Construction in Wisconsin, latest edition, and as specified below.

Set and maintain construction stakes or marks as necessary to achieve the required accuracy and to support the method of operations. Locate stakes to within 0.02 feet of the true horizontal position, and to establish the grade elevation to within 0.01 feet of the true vertical position.

D Measurement

The department will measure Construction Staking Water Main as EACH unit acceptably completed for the entire project.

E Payment

The department will pay for measured quantities at the contract unit price under the following bid item:

ITEM NUMBER DESCRIPTION UNIT

SPV.0060.## Construction Staking Water Main EACH

Payment is full compensation for performing all survey work required to layout and construct all water main work under this contract; and for relocating and resetting damaged or missing construction stakes.

ner-650-035 (20210716)