{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":43,"n_cols":18,"rows_kept":43,"cut":false,"hidden":false,"merged":[[1,17,6,17],[3,12,6,12],[1,1,6,1],[1,2,6,2],[1,3,6,3],[1,4,6,4],[1,5,2,5],[1,6,2,6],[1,8,1,11],[2,8,2,11],[1,7,2,7],[1,12,2,16]]}
[]
[null,"Station","To","Station","Location",450.4,455.06049999999999,460.52229999999997,"HMA",null,null,null,"HMA Pavement 3 HT 58-28 S",null,null,null,null,"Remarks"]
[null,null,null,null,null,null,null,null,"Pavement 4 LT 58-28 S"]
[null,null,null,null,null,"HMA Cold",null,"HMA",null,"PWL","PWL","Incentive ","460.7223          Ton","PWL","PWL","Incentive ","Incentive Density"]
[null,null,null,null,null,"Weather","Tack","Pavement 3",null,"Density","Air ","Density HMA",null,"Density","Air ","Density HMA","HMA Pavement"]
[null,null,null,null,null,"Paving","Coat","LT 58-28 S",460.5224,"Incentive","Voids","Pavement",null,"Incentive","Voids","Pavement","Longitudinal Joints  "]
[null,null,null,null,null,"Ton","GAL","Ton","Ton","Ton*","Ton**","Ton***",null,"Ton*","Ton**","Ton***","LF****"]
[null,"100+00",null,"250+00","RT"]
[null,"250+00",null,"1050+00","RT"]
[]
[]
[]
[]
[null,null,null,"Delete columns you do not need for your specific project this is a template to be manipulated to your specific project"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"* Tonnage is eligible for Incentive Density PWL 460.2005 and Incentive Air Voids 460.2010."]
[null,"** Tonage is eligible for Incentive Air Voids 460.2010. "]
[null,"*** Tonnage is eligible for QMP Density Incentive 460.2000. Wedging & leveling layers are excluded from density testing and density incentive. "]
[null,"**** LF is eligible for Incentive Density HMA Pavement Longitudinal Joints 460.2007"]