**4085-60-71 Work Description**

The proposed project will include the following work:

* 2-Inch mill of existing asphalt and pave 2-inches of HMA pavement
* Concrete Base Patching
* Curb Ramp replacement
* Add shoulder gravel as needed
* Clean Culvert Pipes
* Retie end walls
* Centerline rumble strips
* New pavement markings will be installed
* Existing guardrail installations will be replaced
* Paving to the face of beam guard
* Grading behind EAT’s