**DT 1078 SUPPLEMENT TO UTILITIES**

**POTENTIAL CONFLICTS WITH PLAN**

**& EXISTING HAZARDOUS STRUCTURES**

9150-06-71

STH 32

Breed – Townsend

Parkway Dr (S Jct) – CTH W

Oconto County

Generated by Ken Baierl for DT 1078 Submittal, 2.7.2020

**Potential Utility Conflicts**

|  |  |  |  |
| --- | --- | --- | --- |
| STATION | OFFSET | WORK OCCURRING | UTILITIES IN AREA |
| 206+31 | LT & RT | Remove & replace culvert. New culvert to be longer than existing culvert. | New CP is over fiberoptic on LT and over gas & telephone on RT. |
| 230+64 | RT | Remove culvert headwall and extend culvert. | New CP is over underground electric. |
| 286+89 | LT & RT | Remove headwalls and extend both ends of culvert, utilizing concrete collars to attach. | New CP is over gas line on LT and over telephone line on RT. |
| 310+20 – 311+50 | LT | Installing timber guard posts | Unknown – no field survey of utilities |

**Existing Hazardous Structures**

|  |  |  |  |
| --- | --- | --- | --- |
| DESCRIPTION | STATION | OFFSET | LOCATION REFERENCE |
| Power pole, 11-inch diameter | 205+85 | 37’ LT | 80 feet north of 32 / Pavlat Lane intersection |
| Power pole, 8-inch diameter | 167+10 | 26’ RT | 160 feet south of 32 / Pavlat Lane intersection |