*August 23, 2018*

**NOTICE TO ALL CONTRACTORS:**

|  |  |  |
| --- | --- | --- |
| **Emergency Project:** | **3050-05-70/71** **C. Sun Prairie, Main Street** **Bristol Street Intersection****STH 19** **Dane County** |  |

**Letting of 8/22/2018**

This is Addendum No. 1, which provides for the following:

**Special Provisions:**

|  |
| --- |
| **Revised** Special Provisions |
| ArticleNo. | Description |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

|  |
| --- |
| **Added** Special Provisions |
| ArticleNo. | Description |
| SPV.0090.03 | 30” Curb and Gutter with 8-Inch Curb Height |
|  |  |
|  |  |
|  |  |
|  |  |

|  |
| --- |
| **Deleted** Special Provisions |
| ArticleNo. | Description |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

**Schedule of Items:**

|  |
| --- |
| **Revised** Bid Item Quantities |
| Bid Item | Item Description | Unit | Old Quantity | Revised Quantity | Proposal Total |
| 601.0409 | Concrete Curb & Gutter 30-Inch Type A | LF | 413 | -108 | 305 |
| 601.0411 | Concrete Curb & Gutter 30-Inch Type D | LF | 604 | -88 | 516 |
| 637.2210 | Signs Type II Reflective H | SF | 63.5 | 16 | 79.5 |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

|  |
| --- |
| **Added** Bid Item Quantities |
| Bid Item | Item Description | Unit | Old Quantity | Revised Quantity | Proposal Total |
| 204.9060.S | Removing 01. Existing Street Lights and Poles | EA | 0 | 4 | 4 |
| SPV.0090 – Special 03 | Curb and Gutter with 8-Inch Curb Height | LF | 0 | 196 | 196 |
| 637.2215 | Signs Type II Reflective H Folding | SF | 0 | 18 | 18 |
| 646.7120 | Marking Diagonal Paint 12-Inch | LF | 0 | 46 | 46 |
|  |  |  |  |  |  |

|  |
| --- |
| **Deleted** Bid Item Quantities |
| Bid Item | Item Description | Unit | Old Quantity | Revised Quantity | Proposal Total |
| 204.0110 | Removing Asphaltic Surface | SY | 110 | 0 | 0 |
| 465.0120 | Asphaltic Surface Driveways and Field entrances | Ton | 19 | 0 | 0 |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

**Plan Sheets:**

|  |
| --- |
| **Revised** Plan Sheets |
| Plan Sheet | Plan Sheet Title (brief description of changes to sheet) |
| 3 | Removed driveways behind sidewalk |
| 6,7 | Slope and Width Changes, Added curb and gutter 8-inch |
| 9 | Added curb and gutter 8-inch construction detail |
| 11 | Removed driveways behind sidewalk and added curb and gutter 8-inch |
| 13 | Adjusted storm sewer tap for signal base adjustment |
| 18 | Added R3-8 Signs, Increased folding stop sizes, modified J-Assemblies |
| 21 | Adjusted Signal bases, pullboxes, traffic loops locations |
| 24 | Added marking line epoxy 12-inch in medians, added callouts for arrows |
| 27 | Added note for curb and gutter 8-inch |
| 28 | Added note for curb and gutter 8-inch, adjusted profile, removed driveway behind sidewalk |
| 29 | Removed driveways behind sidewalk, added note for curb and gutter 8-inch |

|  |
| --- |
| **Added** Plan Sheets |
| Plan Sheet | Plan Sheet Title (brief description of why sheet was added) |
| 8 | Curb ramp construction detail |
| 12 | Pavement Grades |
| 63 | Added SDD 15c18-4 |
| 82 | Added Sign Plaque R3-8 and R3-8A |
| 85-102 | Added Cross Sections |

|  |
| --- |
| **Deleted** Plan Sheets |
| Plan Sheet | Plan Sheet Title (brief description of why sheet was deleted) |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

**Other**

*(If necessary, describe any other miscellaneous changes here.)*

The responsibility for notifying potential subcontractors and suppliers of these changes remains with the prime contractor.

Sincerely,

Brad Schultz

Project Manager

**ADDENDUM NO. 1**

**Special Provisions**

1. 30” Curb and Gutter with 8-Inch Curb Height, Item SPV.0090.03.

**A  Description**

This special provision describes providing special curb and gutter along the NE quadrant of the intersection of Bristol St. and Main St. as shown on the plan sheets adjacent to either concrete or asphaltic pavement.

**B  Materials**

Furnish materials conforming to WisDOT standard specification section 601.2.

**C  Construction**

Construct according to WisDOT standard specification section 601.3.  Tie bars needed when adjacent to concrete pavement will be incidental to this bid item.

Construct this 8-Inch curb height at locations shown on the plans and as directed by the engineer.

**D  Measurement**

The department will measure 30” Curb and Gutter with 8-Inch Curb Height by the linear foot acceptably completed adjacent to concrete or asphalt pavements.

**E  Payment**

The department will pay for measured quantities at the contract unit price under the following bid item:

|  |  |  |
| --- | --- | --- |
| ITEM NUMBER | DESCRIPTION | UNIT |
| SPV.0090.03 | 30” Curb and Gutter with 8-Inch Curb Height | LF |

Payment is full compensation for foundation excavation and preparation; special construction required at driveway and alley entrances, or curb ramps; for providing materials, including concrete, expansion joints; for placing, finishing, protecting, and curing; for sawing joints; and for disposing of surplus excavation material, and restoring the work site. However, if the contract provides a bid item for excavation, then the department will pay for excavation required for this work as specified in the contract. Payment also includes providing tie bars in unhardened concrete. For tie bars provided in concrete not placed under the contract, the department will pay separately under the Drilled Tie Bars bid item as specified in 416.5.

The department will adjust pay for crack repairs on concrete built under 601 as specified in 416.5.2 for ancillary concrete.

END OF ADDENDUM